<?xml version="1.0" encoding="utf-8"?>
<JingJiBiao Xmbh="01" Xmmc="上海中医药大学附属曙光医院安徽医院与合肥地铁连接通道工程" Version="1.0" Jsfs="一般计税" Jsdw="安徽省工程咨询研究院（安徽省政府投资项目评审中心）" Zjzmj="0">
  <ZhaoBiaoXx Zbr="安徽省工程咨询研究院（安徽省政府投资项目评审中心）" Zxr="1" ZbrDb="1" ZxrDb="1" Bzr="2" Fhr="1" BzRq="2025-09-11" FhRq="2025-09-11" />
  <Dxgcxx Dxgcmc="上海中医药大学附属曙光医院安徽医院与合肥地铁连接通道工程" Dxgcbh="001" Je="0" Bkjzf="0" Aqwmf="0" Zgj="0" Jzmj="0">
    <Dwgcxx Dwgcbh="0001" Dwgcmc="土建工程" Zylb="1" Jzmj="0" SoftName="国泰新点软件股份有限公司" SoftNum="30A18A095B562D6D2C1A60BC45D89196AA36B4B20D1E3F5B60A95DCE14113946CDB377BA186604044BEEF39BD7C006EF" DogNum="9733c801000702079e12000f002e001e" MachineKey="24418CF90623" Gcszd="市区">
  <Bkjzf>
    <BkjzfMx Xh="1.1" Bm="JF-01" Mc="    环境保护费" Qfjs="0" Fl="3.28" Je="0" Fyxlb="1.1" />
    <BkjzfMx Xh="1.2" Bm="JF-02" Mc="    文明施工费" Qfjs="0" Fl="5.12" Je="0" Fyxlb="1.2" />
    <BkjzfMx Xh="1.3" Bm="JF-03" Mc="    安全施工费" Qfjs="0" Fl="4.13" Je="0" Fyxlb="1.3" />
    <BkjzfMx Xh="1.4" Bm="JF-04" Mc="    临时设施费" Qfjs="0" Fl="8.1" Je="0" Fyxlb="1.4" />
    <BkjzfMx Xh="2.2" Bm="JF-05" Mc="  环境保护税" Qfjs="0" Fl="0" Je="0" Fyxlb="2.2" />
  </Bkjzf>
  <Sj>
    <SjMx Xh="1" Mc="税金" Qfjs="0" Jsjc="分部分项工程费+措施项目费+不可竞争费+其他项目费" Fl="9" Je="0" Fyxlb="1" />
  </Sj>
  <Qdxm>
    <QdBt Bm="0101" Mc="土石方工程" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="1" Qdbm="010101002001" Mc="挖一般土方" Xmtz="1.土壤类别：详见地勘报告，挖土深度综合考虑&#xA;2.挖土深度：详见设计图纸&#xA;3.含现状地表上的地坪、水井、自然坑洞、垃圾池、围挡、现状钢筋混凝土构筑物及圬工构筑物、管网、围墙、拆除后的房屋地坪及基础、因道路施工、房屋拆迁引起的或沿线单位外弃的建筑垃圾和生活垃圾，树木、苗木迁移后的树根、树桩等垃圾、原厂区内原有建构筑物(厂房、围墙等)及其地下基础、地下管线等拆除等&#xA;4.开挖过程中所遇淤泥、障碍物、硬化场地破除、现场局部不平整、部分垃圾处理和清运费用等考虑在报价内，中标后不予调整&#xD;&#xA;5.具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="386.16" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="2" Qdbm="010101002002" Mc="挖一般土方" Xmtz="1.现场场地堆放的土方、建筑垃圾&#xA;2.具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="915.25" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="3" Qdbm="010102001001" Mc="挖一般石方" Xmtz="1．岩石类别：详见地质勘察报告&#xD;&#xA;2．含石方破除、挖运、装车等&#xD;&#xA;3．具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸以体积计算" Dw="m3" Sl="1931.69" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="4" Qdbm="WB010101013001" Mc="余方弃置（土方）" Xmtz="1、运距：弃土运距投标人自行考虑，投标人自行考虑弃土场&#xA;2、投标人需自行勘查现场，投标报价需包含运输费、渣土费、弃土场费、协调费、道路卫生清理费以及市容、路政、环保等部门征收费用等一切费用，中标后不予调整&#xA;3、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按需运输土方，以天然密实体积计算" Dw="m3" Sl="1301.41" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="5" Qdbm="WB010102005001" Mc="余方弃置（石方）" Xmtz="1、运距：运距投标人自行考虑，投标人自行考虑弃石场&#xA;2、投标人需自行勘查现场，投标报价需包含运输费、渣土费、弃土场费、协调费、道路卫生清理费以及市容、路政、环保等部门征收费用等一切费用，中标后不予调整&#xA;3、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按需运输石方，以天然密实体积计算" Dw="m3" Sl="1931.69" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="6" Qdbm="010103001001" Mc="回填方" Xmtz="1、部位：基础回填&#xA;2、密实度要求：满足设计图纸及规范要求&#xA;3、填方材料品种：素土&#xA;4、运距：运距投标人自行考虑&#xA;5、投标人需自行勘查现场，投标报价需包含运输费、渣土费、协调费、道路卫生清理费以及市容、路政、环保等部门征收费用等一切费用，中标后不予调整&#xA;6、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸,以体积计算" Dw="m3" Sl="734.49" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="7" Qdbm="010103001002" Mc="回填方" Xmtz="1、部位：基础回填&#xA;2、密实度要求：满足设计图纸及规范要求&#xA;3、填方材料品种：6%灰土&#xA;4、运距：运距投标人自行考虑&#xA;5、投标人需自行勘查现场，投标报价需包含运输费、渣土费、协调费、道路卫生清理费以及市容、路政、环保等部门征收费用等一切费用，中标后不予调整&#xA;6、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸,以体积计算" Dw="m3" Sl="179.01" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="010202" Mc="基坑与边坡支护" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="8" Qdbm="010202009001" Mc="喷射混凝土" Xmtz="1.厚度：100mm&#xD;&#xA;2.混凝土类别、强度等级：C25喷射混凝土&#xD;&#xA;3.泄水管采用φ50PVC排水管,管壁带孔(外缚双层土工布滤水材料)，泄水管长度在含水层不得小于1.0m，其余土层不得小于0.5m，布置间距满足图纸设计要求&#xD;&#xA;4.具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="762.12" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="9" Qdbm="010202011001" Mc="钢支撑、钢围檩、钢板撑" Xmtz="1.钢材品种、规格：Q235B钢材&#xD;&#xA;2.含钢支撑、钢围檩、钢板撑等制作、安装、拆除&#xD;&#xA;3.含止水片、活络头、钢构件节点板等&#xD;&#xA;4.需考虑残值回收、残值以料抵工&#xD;&#xA;5.具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸，以质量计算" Dw="t" Sl="55.012" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="10" Qdbm="WB010302001001" Mc="灌注混凝土桩钻（挖）孔" Xmtz="1．桩类型：基坑支护桩&#xD;&#xA;2．地层情况：详见地质勘察报告&#xD;&#xA;3．桩径：800mm&#xD;&#xA;4．成孔方法：机械成孔&#xD;&#xA;5．含泥浆运输、钢护筒埋设等&#xD;&#xA;6．具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸从自然地面至桩底，以体积计算" Dw="m3" Sl="360.37" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="11" Qdbm="WB010302002001" Mc="灌注混凝土桩入岩增加费" Xmtz="1．岩石类别：详地质勘查报告&#xD;&#xA;2．桩径：φ800mm&#xD;&#xA;3．成孔方法：机械成孔&#xD;&#xA;4．具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按入岩深度乘以设计桩截面面积，以体积计算" Dw="m3" Sl="292.85" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="12" Qdbm="WB010202012001" Mc="灌注桩混凝土浇筑" Xmtz="1．地层情况：详见地质勘查报告&#xD;&#xA;2．桩长：16.1~18.6m，具体详见设计图纸&#xD;&#xA;3．桩径：φ800mm&#xD;&#xA;4．混凝土（水泥）强度等级：C30水下混凝土&#xD;&#xA;5．含桩身混凝土超灌&#xD;&#xA;6．具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="360.37" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="13" Qdbm="WB010302010001" Mc="钢筋笼制作" Xmtz="1.桩径：φ800mm&#xD;&#xA;2.钢筋种类、规格：HPB300钢筋，φ10&#xD;&#xA;3.具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸，以质量计算" Dw="t" Sl="0.666" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="14" Qdbm="WB010302010002" Mc="钢筋笼制作" Xmtz="1.桩径：φ800mm&#xD;&#xA;2.钢筋种类、规格：HPB300钢筋，φ12&#xD;&#xA;3.具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸，以质量计算" Dw="t" Sl="11.191" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="15" Qdbm="WB010302010003" Mc="钢筋笼制作" Xmtz="1.桩径：φ800mm&#xD;&#xA;2.钢筋种类、规格：HRB400钢筋，φ16&#xD;&#xA;3.具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸，以质量计算" Dw="t" Sl="4.074" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="16" Qdbm="WB010302010004" Mc="钢筋笼制作" Xmtz="1.桩径：φ800mm&#xD;&#xA;2.钢筋种类、规格：HRB400钢筋，φ20&#xD;&#xA;3.具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸，以质量计算" Dw="t" Sl="5.401" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="17" Qdbm="WB010302010005" Mc="钢筋笼制作" Xmtz="1.桩径：φ800mm&#xD;&#xA;2.钢筋种类、规格：HRB400钢筋，φ22&#xD;&#xA;3.具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸，以质量计算" Dw="t" Sl="34.148" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="18" Qdbm="WB010302011001" Mc="钢筋笼安装" Xmtz="1.桩长：25米内&#xD;&#xA;2.具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按安装数量计算" Dw="根" Sl="42" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="19" Qdbm="WB010202014001" Mc="挂钢筋网" Xmtz="1.钢筋种类、规格：钢筋网片采用HPB300φ8@200*200mm，拉筋及加强筋采用HRB400钢筋φ16&#xD;&#xA;2.含支护桩间挂网植筋&#xD;&#xA;3.具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸，以质量计算" Dw="t" Sl="3.205" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="20" Qdbm="010503002001" Mc="冠梁、混凝土支撑、板撑" Xmtz="1．混凝土种类：商品混凝土&#xD;&#xA;2．混凝土强度等级：C30&#xD;&#xA;3．含冠梁、混凝土支撑、板撑、牛腿、围檩等&#xD;&#xA;4．具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="59.19" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="21" Qdbm="011702006001" Mc="冠梁、混凝土支撑、板撑模板" Xmtz="1.支撑高度：投标人自行考虑&#xD;&#xA;2.含冠梁、混凝土支撑、板撑、牛腿、围檩等模板&#xD;&#xA;3.含混凝土模板及支架的制作、安装、拆除、整理堆放、场内外运输费用&#xD;&#xA;4.含清理模板粘结物、杂物、刷隔离剂等一切费用由投标人综合考虑、自行报价&#xD;&#xA;5.具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按模板与现浇混凝土接触面积计算" Dw="m2" Sl="180.64" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="22" Qdbm="010504001001" Mc="挡土墙" Xmtz="1．混凝土种类：商品混凝土&#xD;&#xA;2．混凝土强度等级：C30&#xD;&#xA;3．具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="19.30" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="23" Qdbm="011702011001" Mc="挡土墙模板" Xmtz="1.墙类型：挡土墙&#xD;&#xA;2.含混凝土模板及支架的制作、安装、拆除、整理堆放、场内外运输费用&#xD;&#xA;3.含清理模板粘结物、杂物、刷隔离剂等一切费用由投标人综合考虑、自行报价&#xD;&#xA;4.具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按模板与现浇混凝土接触面积计算" Dw="m2" Sl="128.71" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="24" Qdbm="010507003001" Mc="截水沟" Xmtz="1．断面尺寸：300*300mm&#xD;&#xA;2．混凝土种类：商品混凝土&#xD;&#xA;3．混凝土强度等级：C20&#xD;&#xA;4．具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m" Sl="53.63" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="25" Qdbm="011702026001" Mc="截水沟模板" Xmtz="1.类型：截水沟&#xD;&#xA;2.含混凝土模板及支架的制作、安装、拆除、整理堆放、场内外运输费用&#xD;&#xA;3.含清理模板粘结物、杂物、刷隔离剂等一切费用由投标人综合考虑、自行报价&#xD;&#xA;4.具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按模板与现浇混凝土接触面积计算" Dw="m2" Sl="32.18" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="26" Qdbm="010404001001" Mc="地面硬化" Xmtz="1.材料品种及比例：100mm厚C20混凝土地坪&#xD;&#xA;2.具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m2" Sl="80.45" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="27" Qdbm="011602002001" Mc="钢筋混凝土构件拆除" Xmtz="1．构件名称：混凝土支撑、冠梁、桩头 、原医院地下室的4根支护桩（从桩顶凿除至通道底板下）等&#xD;&#xA;2．含建筑垃圾挖渣、清理及外运&#xD;&#xA;3．具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按拆除部位，以体积计算" Dw="m3" Sl="106.98" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="28" Qdbm="010515001001" Mc="现浇构件钢筋" Xmtz="1、钢筋种类、规格：HPB300  φ8&#xD;&#xA;2、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示钢筋长度乘以单位理论质量计算" Dw="t" Sl="0.560" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="29" Qdbm="010515001002" Mc="现浇构件钢筋" Xmtz="1、钢筋种类、规格：HPB300  φ10&#xD;&#xA;2、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示钢筋长度乘以单位理论质量计算" Dw="t" Sl="1.704" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="30" Qdbm="010515001003" Mc="现浇构件钢筋" Xmtz="1．钢筋种类、规格：HPB300 φ12&#xD;&#xA;2．具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示钢筋长度乘以单位理论质量计算" Dw="t" Sl="1.356" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="31" Qdbm="010515001004" Mc="现浇构件钢筋" Xmtz="1、钢筋种类、规格：HRB400  φ10&#xD;&#xA;2、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示钢筋长度乘以单位理论质量计算" Dw="t" Sl="0.937" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="32" Qdbm="010515001005" Mc="现浇构件钢筋" Xmtz="1、钢筋种类、规格：HRB400  φ12&#xD;&#xA;2、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示钢筋长度乘以单位理论质量计算" Dw="t" Sl="1.258" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="33" Qdbm="010515001006" Mc="现浇构件钢筋" Xmtz="1、钢筋种类、规格：HRB400  φ14&#xD;&#xA;2、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示钢筋长度乘以单位理论质量计算" Dw="t" Sl="0.870" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="34" Qdbm="010515001007" Mc="现浇构件钢筋" Xmtz="1、钢筋种类、规格：HRB400  φ16&#xD;&#xA;2、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示钢筋长度乘以单位理论质量计算" Dw="t" Sl="0.182" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="35" Qdbm="010515001008" Mc="现浇构件钢筋" Xmtz="1、钢筋种类、规格：HRB400  φ20&#xD;&#xA;2、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示钢筋长度乘以单位理论质量计算" Dw="t" Sl="1.758" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="36" Qdbm="010515001009" Mc="现浇构件钢筋" Xmtz="1、钢筋种类、规格：HRB400  φ22&#xD;&#xA;2、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示钢筋长度乘以单位理论质量计算" Dw="t" Sl="3.464" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="37" Qdbm="010515001010" Mc="现浇构件钢筋" Xmtz="1、钢筋种类、规格：HRB400  φ25&#xD;&#xA;2、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示钢筋长度乘以单位理论质量计算" Dw="t" Sl="1.703" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="0104" Mc="砌筑工程" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="38" Qdbm="010401001001" Mc="砖基础" Xmtz="1．部位：砖胎膜、底板侧边永久砖墙和临时砖墙&#xD;&#xA;2．砖品种、规格、强度级：蒸压灰砂砖，强度等级不小于MU15&#xD;&#xA;3．砂浆强度级：DM M7.5预拌砂浆&#xD;&#xA;4.  抹灰：20mm厚1:2水泥砂浆找平层&#xD;&#xA;5．具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="8.37" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="39" Qdbm="010401003001" Mc="实心砖墙" Xmtz="1.砖品种、规格、强度级：蒸压灰砂砖，强度等级不小于MU15&#xD;&#xA;2.墙厚：200mm&#xD;&#xA;3.砂浆强度：DM M7.5预拌砂浆&#xD;&#xA;4.高度3.6m以内&#xD;&#xA;5.具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="1.70" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="40" Qdbm="010401003002" Mc="实心砖墙" Xmtz="1.砖品种、规格、强度级：蒸压灰砂砖，强度等级不小于MU15&#xD;&#xA;2.墙厚：200mm&#xD;&#xA;3.砂浆强度：DM M7.5水泥砂浆&#xD;&#xA;4.高度3.6m以外&#xD;&#xA;5.具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="3.66" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="41" Qdbm="010401003003" Mc="实心砖墙" Xmtz="1.砖品种、规格、强度级：蒸压灰砂砖，强度等级不小于MU15&#xD;&#xA;2.墙厚：300mm&#xD;&#xA;3.砂浆强度： DM M7.5水泥砂浆&#xD;&#xA;4.高度3.6m以内&#xD;&#xA;5.具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="5.65" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="42" Qdbm="010401003004" Mc="实心砖墙" Xmtz="1.砖品种、规格、强度级：蒸压灰砂砖，强度等级不小于MU15&#xD;&#xA;2.墙厚：300mm&#xD;&#xA;3.砂浆强度：DM M7.5水泥砂浆&#xD;&#xA;4.高度3.6m以外&#xD;&#xA;5.具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="11.12" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="43" Qdbm="011601001001" Mc="砖砌体拆除" Xmtz="1．砌体名称：临时砖墙&#xD;&#xA;2．砌体材质：砖砌体&#xD;&#xA;3．砌体表面的附着物种类：水泥砂浆抹灰层&#xD;&#xA;4．含建筑垃圾清理、外运等&#xD;&#xA;5．具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按拆除部位，以体积计算" Dw="m3" Sl="3.86" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="0105" Mc="混凝土工程" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="44" Qdbm="010404001002" Mc="基础垫层" Xmtz="1．厚度：150mm&#xD;&#xA;2．材料品种及比例：C20混凝土垫层&#xD;&#xA;3．具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="32.97" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="45" Qdbm="010404001003" Mc="混凝土回填" Xmtz="1.部位：集水井开挖放坡处&#xD;&#xA;2.材料品种及比例：C20混凝土回填&#xD;&#xA;3.具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="24.80" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="46" Qdbm="010501004001" Mc="现浇混凝土底板" Xmtz="1．混凝土种类：商品混凝土&#xD;&#xA;2．混凝土强度等级：C35 P8&#xD;&#xA;3．含底板排水沟、集水坑工程量&#xD;&#xA;4．具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="177.79" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="47" Qdbm="010503001001" Mc="基础梁" Xmtz="1．混凝土种类：商品混凝土&#xD;&#xA;2．混凝土强度等级：C35 P8&#xD;&#xA;3．具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="3.58" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="48" Qdbm="010502001001" Mc="矩形柱" Xmtz="1．柱规格形状：矩形柱周长1.6m以内&#xD;&#xA;2．混凝土种类：商品混凝土&#xD;&#xA;3．混凝土强度等级：C35&#xD;&#xA;4．含梯柱工程量&#xD;&#xA;5．具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="7.69" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="49" Qdbm="010502002001" Mc="构造柱" Xmtz="1、混凝土种类：商品混凝土&#xD;&#xA;2、混凝土强度等级：C25&#xD;&#xA;3、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="2.17" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="50" Qdbm="010503004001" Mc="圈梁" Xmtz="1.部位：防水反坎、圈梁&#xD;&#xA;2.混凝土种类：商品混凝土&#xD;&#xA;3.混凝土强度等级：C25&#xD;&#xA;4.具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="0.81" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="51" Qdbm="010503005001" Mc="过梁" Xmtz="1、混凝土种类：商品混凝土&#xD;&#xA;2、混凝土强度等级：C25&#xD;&#xA;3、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="0.09" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="52" Qdbm="010504001002" Mc="直形墙" Xmtz="1．墙规格：地下混凝土墙，250厚以上&#xD;&#xA;2．混凝土种类：商品混凝土&#xD;&#xA;3．混凝土强度等级：C35 P8&#xD;&#xA;4．具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="341.69" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="53" Qdbm="010504001003" Mc="直形墙" Xmtz="1．墙规格：地上混凝土墙，200厚以上&#xD;&#xA;2．混凝土种类：商品混凝土&#xD;&#xA;3．混凝土强度等级：C35&#xD;&#xA;4．具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="36.01" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="54" Qdbm="010505002001" Mc="无梁板" Xmtz="1．混凝土种类：商品混凝土&#xD;&#xA;2．混凝土强度等级：C35 P8&#xD;&#xA;3．具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="135.01" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="55" Qdbm="010506001001" Mc="直形楼梯" Xmtz="1．混凝土种类：商品混凝土&#xD;&#xA;2．混凝土强度等级：C35&#xD;&#xA;3．具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸，以水平投影面积计算" Dw="m2" Sl="89.72" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="56" Qdbm="010515001011" Mc="现浇构件钢筋" Xmtz="1、砖墙拉结筋&#xD;&#xA;2、钢筋种类、规格：HPB300  φ6&#xD;&#xA;3、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示钢筋长度乘以单位理论质量计算" Dw="t" Sl="0.331" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="57" Qdbm="010515001012" Mc="现浇构件钢筋" Xmtz="1、钢筋种类、规格：HPB300  φ6&#xD;&#xA;2、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示钢筋长度乘以单位理论质量计算" Dw="t" Sl="0.001" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="58" Qdbm="010515001013" Mc="现浇构件钢筋" Xmtz="1、钢筋种类、规格：HPB300  φ8&#xD;&#xA;2、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示钢筋长度乘以单位理论质量计算" Dw="t" Sl="3.316" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="59" Qdbm="010515001014" Mc="现浇构件钢筋" Xmtz="1、钢筋种类、规格：HPB300  φ10&#xD;&#xA;2、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示钢筋长度乘以单位理论质量计算" Dw="t" Sl="1.038" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="60" Qdbm="010515001015" Mc="现浇构件钢筋" Xmtz="1、钢筋种类、规格：HRB400E  φ8&#xD;&#xA;2、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示钢筋长度乘以单位理论质量计算" Dw="t" Sl="0.632" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="61" Qdbm="010515001016" Mc="现浇构件钢筋" Xmtz="1、钢筋种类、规格：HRB400E  φ12&#xD;&#xA;2、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示钢筋长度乘以单位理论质量计算" Dw="t" Sl="0.783" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="62" Qdbm="010515001017" Mc="现浇构件钢筋" Xmtz="1、钢筋种类、规格：HRB400E  φ14&#xD;&#xA;2、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示钢筋长度乘以单位理论质量计算" Dw="t" Sl="4.798" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="63" Qdbm="010515001018" Mc="现浇构件钢筋" Xmtz="1、钢筋种类、规格：HRB400E  φ16&#xD;&#xA;2、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示钢筋长度乘以单位理论质量计算" Dw="t" Sl="31.470" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="64" Qdbm="010515001019" Mc="现浇构件钢筋" Xmtz="1、钢筋种类、规格：HRB400E  φ18&#xD;&#xA;2、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示钢筋长度乘以单位理论质量计算" Dw="t" Sl="11.799" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="65" Qdbm="010515001020" Mc="现浇构件钢筋" Xmtz="1、钢筋种类、规格：HRB400E  φ20&#xD;&#xA;2、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示钢筋长度乘以单位理论质量计算" Dw="t" Sl="1.417" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="66" Qdbm="010515001021" Mc="现浇构件钢筋" Xmtz="1、钢筋种类、规格：HRB400E  φ22&#xD;&#xA;2、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示钢筋长度乘以单位理论质量计算" Dw="t" Sl="54.080" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="67" Qdbm="010515001022" Mc="现浇构件钢筋" Xmtz="1、钢筋种类、规格：HRB400E  φ25&#xD;&#xA;2、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示钢筋长度乘以单位理论质量计算" Dw="t" Sl="9.243" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="68" Qdbm="010515001023" Mc="现浇构件钢筋" Xmtz="1、钢筋种类、规格：HRB400E  φ28&#xD;&#xA;2、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示钢筋长度乘以单位理论质量计算" Dw="t" Sl="4.398" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="69" Qdbm="010516003001" Mc="钢筋连接" Xmtz="1.规格：综合考虑&#xD;&#xA;2.连接方式：直螺纹连接&#xD;&#xA;3.具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按实际数量计算" Dw="个" Sl="2181" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="0106" Mc="金属结构工程" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="70" Qdbm="010606008001" Mc="钢梯" Xmtz="1．部位：集水井钢爬梯&#xD;&#xA;2．钢梯形式：圆钢φ30@300mm、两端打扁砌入墙内&#xD;&#xA;3．具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸，以质量计算" Dw="t" Sl="0.031" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="0109" Mc="屋面及防水工程" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="71" Qdbm="010904001001" Mc="楼（地）面卷材防水" Xmtz="1．部位：底板&#xD;&#xA;2．卷材品种、规格、厚度：1.5mm厚自粘聚合物改性沥青卷材(无胎 )&#xD;&#xA;3．防水加强层综合考虑在报价中，中标后不予调整&#xD;&#xA;4．具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="297.75" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="72" Qdbm="010904001002" Mc="楼（地）面卷材防水" Xmtz="1．部位：底板&#xD;&#xA;2．卷材品种、规格、厚度：1.5mm厚预铺高分子(非沥青基)防水卷材P类&#xD;&#xA;3．防水加强层综合考虑在报价中，中标后不予调整&#xD;&#xA;4．具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="297.75" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="73" Qdbm="010903001001" Mc="墙面卷材防水" Xmtz="1．部位：侧壁&#xD;&#xA;2．卷材品种、规格、厚度：1.5mm厚自粘聚合物改性沥青卷材(无胎 )&#xD;&#xA;3.   防水加强层综合考虑在报价中，中标后不予调整&#xD;&#xA;4．具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="473.56" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="74" Qdbm="010903001002" Mc="墙面卷材防水" Xmtz="1．部位：侧壁&#xD;&#xA;2．卷材品种、规格、厚度：1.5mm厚预铺高分子(非沥青基)防水卷材P类&#xD;&#xA;3.   防水加强层综合考虑在报价中，中标后不予调整&#xD;&#xA;4．具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="473.56" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="75" Qdbm="010902001001" Mc="屋面卷材防水" Xmtz="1．部位：顶板&#xD;&#xA;2．卷材品种、规格、厚度：4mm厚自粘聚合物改性沥青防水卷材PY-Ⅱ&#xD;&#xA;3．防水加强层综合考虑在报价中，中标后不予调整&#xD;&#xA;4．具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="214.49" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="76" Qdbm="010902002001" Mc="屋面涂膜防水" Xmtz="1．部位：顶板&#xD;&#xA;2．防水膜品种：2mm厚非固化橡胶沥青防水涂料&#xD;&#xA;3．防水加强层综合考虑在报价中，中标后不予调整&#xD;&#xA;4．具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="214.49" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="77" Qdbm="010902003001" Mc="屋面刚性层" Xmtz="1．部位：顶板&#xD;&#xA;2．刚性层厚度：70mmC20细石混凝土保护层&#xD;&#xA;3．具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="171.54" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="78" Qdbm="010903004001" Mc="钢板止水带" Xmtz="1．部位：施工缝&#xD;&#xA;2．止水带材料种类：300*4mm钢板止水带&#xD;&#xA;3．含遇水膨胀止水胶20mm×10mm&#xD;&#xA;4．具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸，以长度计算" Dw="m" Sl="126.84" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="79" Qdbm="010904004001" Mc="变形缝" Xmtz="1．部位：顶板、外墙、底板变形缝&#xD;&#xA;2．嵌缝材料：橡胶止水带&#xD;&#xA;3．含遇水膨胀止水胶10mm×5mm及接水盒&#xD;&#xA;4．具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸，以长度计算" Dw="m" Sl="40.60" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="80" Qdbm="010904004002" Mc="变形缝" Xmtz="1．嵌缝材料种类：变形缝衬垫板、泡沫棒、高模量聚氨酯密封胶&#xD;&#xA;2．部位：底板、侧墙、顶板变形缝背水面&#xD;&#xA;3．具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸，以长度计算" Dw="m" Sl="40.60" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="81" Qdbm="010904002001" Mc="涂膜防水" Xmtz="1．部位：施工缝处&#xD;&#xA;2．防水膜品种：2.0厚水泥基渗透结晶防水涂料(1.5kg/m2)&#xD;&#xA;3．具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="79.21" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="82" Qdbm="010904002002" Mc="涂膜防水" Xmtz="1．部位：排水沟和集水井侧壁及底面&#xD;&#xA;2．防水膜品种：2.0厚水泥基渗透结晶防水涂料(1.5kg/m2)&#xD;&#xA;3．具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="34.54" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="83" Qdbm="010904003001" Mc="砂浆防水（防潮）" Xmtz="1．部位：集水坑、排水沟底面及侧壁&#xD;&#xA;2．防水层做法：聚合物水泥防水砂浆(10mm厚)&#xD;&#xA;3．具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="34.54" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="84" Qdbm="010904003002" Mc="砂浆防水（防潮）" Xmtz="1．部位：通道内两侧排水沟底面及侧壁&#xD;&#xA;2．防水层做法：聚合物水泥防水砂浆(20mm厚)&#xD;&#xA;3．具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="41.84" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="85" Qdbm="WB010302008001" Mc="注浆管埋设及注浆" Xmtz="1．管材料、规格：DN40钢管&#xD;&#xA;2．具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计桩长加20cm，以长度计算" Dw="项" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="0117" Mc="措施项目" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="86" Qdbm="011701002001" Mc="外脚手架" Xmtz="1.部位：外墙脚手架&#xD;&#xA;2.搭设方式：投标单位依据施工组织设计方案及相关规范综合考虑&#xD;&#xA;3.脚手架材质：满足合肥市相关文件规定，投标单位依据施工组织设计方案及相关规范综合考虑&#xD;&#xA;4.投标单位根据现有的图纸资料、招标文件和施工规范等资料，必须满足合肥市相关文件规定，综合报价&#xD;&#xA;5.具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按外墙中心线乘以高度的垂直投影面积计算" Dw="m2" Sl="419.85" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="87" Qdbm="WB011701009001" Mc="工具式脚手架" Xmtz="1.高度3.6m以内砌筑脚手架、现浇剪力墙脚手架&#xD;&#xA;2.脚手架材质：满足合肥市相关文件规定，投标单位依据施工组织设计方案及相关规范综合考虑&#xD;&#xA;3.投标单位根据现有的图纸资料、招标文件和施工规范等资料，必须满足合肥市相关文件规定，综合报价&#xD;&#xA;4.具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按实际搭设的水平投影面积计算" Dw="m2" Sl="90.45" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="88" Qdbm="WB011701009002" Mc="工具式脚手架" Xmtz="1.高度3.6m以外砌筑脚手架、现浇剪力墙脚手架&#xD;&#xA;2.脚手架材质：满足合肥市相关文件规定，投标单位依据施工组织设计方案及相关规范综合考虑&#xD;&#xA;3.投标单位根据现有的图纸资料、招标文件和施工规范等资料，必须满足合肥市相关文件规定，综合报价&#xD;&#xA;4.具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按实际搭设的水平投影面积计算" Dw="m2" Sl="135.68" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="89" Qdbm="011701006002" Mc="满堂脚手架" Xmtz="1.部位：基础满堂脚手架&#xD;&#xA;2.搭设高度：详见图纸，综合考虑&#xD;&#xA;3.脚手架材质：满足合肥市相关文件规定，投标单位依据施工组织设计方案及相关规范综合考虑&#xD;&#xA;4.投标单位根据现有的图纸资料、招标文件和施工规范等资料，必须满足合肥市相关文件规定，综合报价&#xD;&#xA;5.具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按实际搭设的水平投影面积计算" Dw="m2" Sl="233.10" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="90" Qdbm="011702001001" Mc="基础" Xmtz="1.基础类型：垫层模板&#xD;&#xA;2.含混凝土模板及支架的制作、安装、拆除、整理堆放、场内外运输费用&#xD;&#xA;3.含清理模板粘结物、杂物、刷隔离剂等一切费用由投标人综合考虑、自行报价&#xD;&#xA;4.具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按模板与现浇混凝土接触面积计算" Dw="m2" Sl="20.65" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="91" Qdbm="011702001002" Mc="基础" Xmtz="1.基础类型：集水坑模板&#xD;&#xA;2.含混凝土模板及支架的制作、安装、拆除、整理堆放、场内外运输费用&#xD;&#xA;3.含清理模板粘结物、杂物、刷隔离剂等一切费用由投标人综合考虑、自行报价&#xD;&#xA;4.具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按模板与现浇混凝土接触面积计算" Dw="m2" Sl="27.50" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="92" Qdbm="011702005001" Mc="基础梁" Xmtz="1．类型：基础梁&#xD;&#xA;2.含混凝土模板及支架的制作、安装、拆除、整理堆放、场内外运输费用&#xD;&#xA;3.含清理模板粘结物、杂物、刷隔离剂等一切费用由投标人综合考虑、自行报价&#xD;&#xA;4.具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按模板与现浇混凝土接触面积计算" Dw="m2" Sl="13.74" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="93" Qdbm="011702002001" Mc="矩形柱" Xmtz="1．柱截面尺寸：矩形柱，周长1.6m以内&#xD;&#xA;2.含混凝土模板及支架的制作、安装、拆除、整理堆放、场内外运输费用&#xD;&#xA;3.含清理模板粘结物、杂物、刷隔离剂等一切费用由投标人综合考虑、自行报价&#xD;&#xA;4.具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按模板与现浇混凝土接触面积计算" Dw="m2" Sl="59.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="94" Qdbm="011702003001" Mc="构造柱" Xmtz="1、构造柱模板&#xD;&#xA;2.含混凝土模板及支架的制作、安装、拆除、整理堆放、场内外运输费用&#xD;&#xA;3.含清理模板粘结物、杂物、刷隔离剂等一切费用由投标人综合考虑、自行报价&#xD;&#xA;4.具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按模板与现浇混凝土接触面积计算" Dw="m2" Sl="17.99" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="95" Qdbm="011702008001" Mc="圈梁" Xmtz="1．圈梁模板&#xD;&#xA;2.含混凝土模板及支架的制作、安装、拆除、整理堆放、场内外运输费用&#xD;&#xA;3.含清理模板粘结物、杂物、刷隔离剂等一切费用由投标人综合考虑、自行报价&#xD;&#xA;4.具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按模板与现浇混凝土接触面积计算" Dw="m2" Sl="6.96" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="96" Qdbm="011702009001" Mc="过梁" Xmtz="1、过梁模板&#xD;&#xA;2.含混凝土模板及支架的制作、安装、拆除、整理堆放、场内外运输费用&#xD;&#xA;3.含清理模板粘结物、杂物、刷隔离剂等一切费用由投标人综合考虑、自行报价&#xD;&#xA;4.具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按模板与现浇混凝土接触面积计算" Dw="m2" Sl="1.25" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="97" Qdbm="011702011002" Mc="直形墙" Xmtz="1.墙类型：地下混凝土墙模板&#xD;&#xA;2.含混凝土模板及支架的制作、安装、拆除、整理堆放、场内外运输费用&#xD;&#xA;3.含清理模板粘结物、杂物、刷隔离剂等一切费用由投标人综合考虑、自行报价&#xD;&#xA;4.具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按模板与现浇混凝土接触面积计算" Dw="m2" Sl="1188.67" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="98" Qdbm="011702011003" Mc="直形墙" Xmtz="1．墙类型：地上混凝土墙模板&#xD;&#xA;2.  含混凝土模板及支架的制作、安装、拆除、整理堆放、场内外运输费用&#xD;&#xA;3.  含清理模板粘结物、杂物、刷隔离剂等一切费用由投标人综合考虑、自行报价&#xD;&#xA;4.  具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按模板与现浇混凝土接触面积计算" Dw="m2" Sl="240.01" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="99" Qdbm="011702014001" Mc="顶板" Xmtz="1.类型：通道顶板模板&#xD;&#xA;2.含混凝土模板及支架的制作、安装、拆除、整理堆放、场内外运输费用&#xD;&#xA;3.含清理模板粘结物、杂物、刷隔离剂等一切费用由投标人综合考虑、自行报价&#xD;&#xA;4.具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按模板与现浇混凝土接触面积计算" Dw="m2" Sl="167.19" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="100" Qdbm="WB011702030001" Mc="柱支模超高" Xmtz="1、柱支模超高&#xD;&#xA;2、具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按超出3.6m部分的模板与现浇混凝土接触面积计算" Dw="m2" Sl="81.08" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="101" Qdbm="WB011702032001" Mc="墙支模超高" Xmtz="1.墙类型：通道侧壁模板&#xD;&#xA;2.含混凝土模板及支架的制作、安装、拆除、整理堆放、场内外运输费用&#xD;&#xA;3.含清理模板粘结物、杂物、刷隔离剂等一切费用由投标人综合考虑、自行报价&#xD;&#xA;4.具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按超出3.6m部分的模板与现浇混凝土接触面积计算" Dw="m2" Sl="2741.95" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="102" Qdbm="WB011702033001" Mc="板支模超高" Xmtz="1.类型：通道顶板模板&#xD;&#xA;2.含混凝土模板及支架的制作、安装、拆除、整理堆放、场内外运输费用&#xD;&#xA;3.含清理模板粘结物、杂物、刷隔离剂等一切费用由投标人综合考虑、自行报价&#xD;&#xA;4.具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按超出3.6m部分的模板与现浇混凝土接触面积计算" Dw="m2" Sl="585.42" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="103" Qdbm="011702024001" Mc="楼梯" Xmtz="1.类型：直型楼梯&#xD;&#xA;2.含混凝土模板及支架的制作、安装、拆除、整理堆放、场内外运输费用&#xD;&#xA;3.含清理模板粘结物、杂物、刷隔离剂等一切费用由投标人综合考虑、自行报价&#xD;&#xA;4.具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按楼梯（包括休息平台、水平梁、斜梁和楼层板的连接梁）的水平投影面积计算" Dw="m2" Sl="89.72" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="104" Qdbm="011702026002" Mc="电缆沟、地沟" Xmtz="1.类型：排水沟、截水沟&#xD;&#xA;2.含混凝土模板及支架的制作、安装、拆除、整理堆放、场内外运输费用&#xD;&#xA;3.含清理模板粘结物、杂物、刷隔离剂等一切费用由投标人综合考虑、自行报价&#xD;&#xA;4.具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按模板与现浇混凝土接触面积计算" Dw="m2" Sl="2.52" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="105" Qdbm="011702027001" Mc="台阶" Xmtz="1.类型：台阶&#xD;&#xA;2.含混凝土模板及支架的制作、安装、拆除、整理堆放、场内外运输费用&#xD;&#xA;3.含清理模板粘结物、杂物、刷隔离剂等一切费用由投标人综合考虑、自行报价&#xD;&#xA;4.具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按图示台阶水平投影面积计算" Dw="m2" Sl="3.86" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="106" Qdbm="011703001001" Mc="垂直运输" Xmtz="1．建筑物檐口高度、层数：详见图纸&#xD;&#xA;2．投标单位根据现有的图纸资料、招标文件和施工规范等资料，充分考虑，一次性报价，中标后不得调整" Gcnr="" Jsgz="1.建筑物地下室部分垂直运输按设计室内地坪(±0.00)以下的建筑面积，以面积计算2.建筑物上部建筑部分垂直运输按室内地坪(±0.00)以上的建筑面积总和，以面积计算" Dw="项" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="107" Qdbm="WB011706003001" Mc="降水、排水" Xmtz="1．机械规格型号：自行考虑&#xD;&#xA;2．投标单位根据现有的图纸资料、招标文件和施工规范等资料，充分考虑，一次性报价，中标后不得调整" Gcnr="" Jsgz="按地质报告说明的地下水位以下的需排水的地下室的建筑面积计算" Dw="项" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="3" Mc="其他" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="108" Qdbm="011705001001" Mc="大型机械设备进出场及安拆" Xmtz="1．机械设备名称：含连接通道施工所用到的所有大型机械的进出场及安拆费&#xD;&#xA;2．具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按使用机械设备的数量计算" Dw="项" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="109" Qdbm="WB010202012002" Mc="桩基检测" Xmtz="1．围护桩应采用低应变动测法检测桩身完整性,检测数量不应少于总桩数的20%且不少于5根&#xD;&#xA;2.   投标人需综合考虑报价，中标后不予调整&#xD;&#xA;3．具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="项" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="110" Qdbm="WB010202012003" Mc="施工监测、监控" Xmtz="1．包括但不限于沉降观测、水平竖向位移监测、变形观测、水位监测、支撑轴力监测等&#xD;&#xA;2.   详见监控量测设计表，投标人需综合考虑报价，中标后不予调整&#xD;&#xA;3．具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="项" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
  </Qdxm>
  <Csxm>
    <ZjCs>
      <ZjCsMx Xh="1" Xmbm="JC-01" Mc="夜间施工增加费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0.5" Je="0" Bz="" Cslb="1" />
      <ZjCsMx Xh="2" Xmbm="JC-02" Mc="二次搬运费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="1" Je="0" Bz="" Cslb="2" />
      <ZjCsMx Xh="3" Xmbm="JC-03" Mc="冬雨季施工增加费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0.8" Je="0" Bz="" Cslb="3" />
      <ZjCsMx Xh="4" Xmbm="JC-04" Mc="已完工程及设备保护费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0.1" Je="0" Bz="" Cslb="4" />
      <ZjCsMx Xh="5" Xmbm="JC-05" Mc="工程定位复测费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="1" Je="0" Bz="" Cslb="5" />
      <ZjCsMx Xh="6" Xmbm="JC-06" Mc="非夜间施工照明费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0" Je="0" Bz="" Cslb="6" />
      <ZjCsMx Xh="7" Xmbm="JC-07" Mc="临时保护设施费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0.2" Je="0" Bz="" Cslb="7" />
      <ZjCsMx Xh="8" Xmbm="JC-08" Mc="赶工措施费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0" Je="0" Bz="" Cslb="8" />
    </ZjCs>
  </Csxm>
  <Qtxm>
    <QtxmMx Xh="1" Mc="暂列金额" Dw="项" Je="0" Bz="" Xmlb="1" />
    <QtxmMx Xh="2" Mc="专业工程暂估价" Dw="项" Je="0" Bz="" Xmlb="2" />
    <QtxmMx Xh="3" Mc="计日工" Dw="" Je="0" Bz="" Xmlb="3" />
    <QtxmMx Xh="4" Mc="总承包服务费" Dw="" Je="0" Bz="" Xmlb="4" />
  </Qtxm>
  <Zlje />
  <Clzg />
  <Zygczg />
  <Jrg>
    <JrgBt Xh="一" Mc="人工" Je="0" Lb="1" />
    <JrgBt Xh="二" Mc="材料" Je="0" Lb="2" />
    <JrgBt Xh="三" Mc="施工机械" Je="0" Lb="3" />
  </Jrg>
  <Zcbfwf>
    <ZcbfwfMx Xh="1" Mc="发包人发包专业工程" Xmjz="0" Fwnr="" Fl="0" Je="0" />
    <ZcbfwfMx Xh="2" Mc="发包人供应材料" Xmjz="0" Fwnr="" Fl="0" Je="0" />
  </Zcbfwf>
  <Fbrgycl />
  <CbrgyclCef />
</Dwgcxx>
    <Dwgcxx Dwgcbh="0002" Dwgcmc="装饰工程" Zylb="1" Jzmj="0" SoftName="国泰新点软件股份有限公司" SoftNum="30A18A095B562D6D2C1A60BC45D89196AA36B4B20D1E3F5B60A95DCE14113946CDB377BA18660404B24A150BA5AAE4DE" DogNum="9733c801000702079e12000f002e001e" MachineKey="24418CF90623" Gcszd="市区">
  <Bkjzf>
    <BkjzfMx Xh="1.1" Bm="JF-01" Mc="    环境保护费" Qfjs="0" Fl="3.28" Je="0" Fyxlb="1.1" />
    <BkjzfMx Xh="1.2" Bm="JF-02" Mc="    文明施工费" Qfjs="0" Fl="5.12" Je="0" Fyxlb="1.2" />
    <BkjzfMx Xh="1.3" Bm="JF-03" Mc="    安全施工费" Qfjs="0" Fl="4.13" Je="0" Fyxlb="1.3" />
    <BkjzfMx Xh="1.4" Bm="JF-04" Mc="    临时设施费" Qfjs="0" Fl="8.1" Je="0" Fyxlb="1.4" />
    <BkjzfMx Xh="2.2" Bm="JF-05" Mc="  环境保护税" Qfjs="0" Fl="0" Je="0" Fyxlb="2.2" />
  </Bkjzf>
  <Sj>
    <SjMx Xh="1" Mc="税金" Qfjs="0" Jsjc="分部分项工程费+措施项目费+不可竞争费+其他项目费" Fl="9" Je="0" Fyxlb="1" />
  </Sj>
  <Qdxm>
    <QdBt Bm="0108" Mc="门窗工程" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="1" Qdbm="010802003001" Mc="钢质甲级防火门" Xmtz="1.门类型：钢质甲级防火门&#xD;&#xA;2.白色烤漆钢质防火门框、门饰面&#xD;&#xA;3.包含门套、门框等&#xD;&#xA;4.五金品种、规格：含门锁、闭门器、顺位器等所有五金&#xD;&#xA;5.选用消防部门认可的合格产品&#xD;&#xA;6.具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示洞口尺寸，以面积计算" Dw="m2" Sl="13.11" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="2" Qdbm="010803002001" Mc="防火、管理卷帘门" Xmtz="1．门代号及洞口尺寸：详见设计图纸&#xD;&#xA;2．门材质：双轨无机布基特级防火卷帘门&#xD;&#xA;3．含手动启闭、电动启闭装置，就近电源接入等&#xD;&#xA;4.  具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图纸安装高度乘以门的实际宽度,以面积计算" Dw="m2" Sl="21.60" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="3" Qdbm="010807001001" Mc="金属窗 " Xmtz="1．窗代号及洞口尺寸：可开启排烟窗&#xD;&#xA;2．窗材质：80系列断热铝合金窗&#xD;&#xA;3．玻璃品种、厚度：6low-e+12A+6low-e钢化中空玻璃&#xD;&#xA;4．含电动开窗机、控制箱、控制箱至开窗机设备之间的配电线缆及控制电缆，线缆保护套管、手动开启装置等，并于消防联动&#xD;&#xA;5．具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示洞口尺寸，以面积计算" Dw="m2" Sl="2.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="4" Qdbm="010807003001" Mc="金属百页" Xmtz="1．窗代号及洞口尺寸：详见设计图纸&#xD;&#xA;2．窗材质：铝合金通风百叶，表面氟碳喷涂&#xD;&#xA;3．具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示洞口尺寸，以面积计算" Dw="m2" Sl="2.83" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="0111" Mc="楼地面装饰工程" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="5" Qdbm="011102001001" Mc="石材楼地面" Xmtz="1．800x800x25mm厚白麻花岗岩背刷界面处理剂,白水泥浆擦缝（酸洗打蜡）&#xD;&#xA;2．聚合物改性水泥基粘结剂&#xD;&#xA;3．25厚DSM15预拌砂浆,撒素水泥面(洒适量清水)&#xD;&#xA;4．水泥浆一道(内掺建筑胶)&#xD;&#xA;5．100厚C20混凝土垫层&#xD;&#xA;6．具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="220.96" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="6" Qdbm="011102001002" Mc="石材楼地面" Xmtz="1．400x400x25mm厚灰麻盲道花岗岩背刷界面处理剂,白水泥浆擦缝（酸洗打蜡）&#xD;&#xA;2．含不锈钢盲道条&#xD;&#xA;3．聚合物改性水泥基粘结剂&#xD;&#xA;4．25厚DSM15预拌砂浆,撒素水泥面(洒适量清水)&#xD;&#xA;5．水泥浆一道(内掺建筑胶)&#xD;&#xA;6．100厚C20混凝土垫层&#xD;&#xA;7．具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="22.61" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="7" Qdbm="011102003001" Mc="块料楼地面" Xmtz="1．600*600*10厚防滑地砖,干水泥擦缝&#xD;&#xA;2．25厚DS M15预拌砂浆粘接层铺实拍平&#xD;&#xA;3．C20细石混凝土垫层&#xD;&#xA;4．素水泥浆一道&#xD;&#xA;5．具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="61.91" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="8" Qdbm="011106002001" Mc="块料楼梯面层 " Xmtz="1.部位：楼梯面层&#xD;&#xA;2.600*600*10厚防滑梯级缸砖,干水泥擦缝&#xD;&#xA;3.25厚DS M15预拌砂浆粘接层铺实拍平&#xD;&#xA;4.水泥浆一道,内掺建筑胶&#xD;&#xA;5.具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸，以楼梯（包括踏步、休息平台及≤500mm的楼梯井）水平投影面积计算" Dw="m2" Sl="89.72" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="9" Qdbm="WB011105006001" Mc="成品踢脚线 " Xmtz="1.踢脚线高度：100mm&#xD;&#xA;2.2.0厚深灰色不锈钢踢脚（304#）&#xD;&#xA;3.9厘玻镁板基层&#xD;&#xA;4.界面剂一道&#xD;&#xA;5.具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸，以长度计算" Dw="m" Sl="119.54" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="10" Qdbm="011105003001" Mc="块料踢脚线 " Xmtz="1．踢脚线高度：100mm高&#xD;&#xA;2．面层材料品种、规格、颜色：600*100*8厚地砖踢脚&#xD;&#xA;3．粘贴层厚度、材料种类：9厚DP M20预拌砂浆结合层(内掺建筑胶)&#xD;&#xA;4．刷素水泥浆一道(内掺建筑胶)&#xD;&#xA;5．具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸，以长度计算" Dw="m" Sl="164.71" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="11" Qdbm="011107001001" Mc="石材台阶面 " Xmtz="1．面层材料品种、规格、颜色：25厚白麻烧面花岗岩&#xD;&#xA;2．粘结层材料种类：25厚1:3干硬性水泥砂浆粘接层，上撒素水泥&#xD;&#xA;3．素水泥浆一道（内掺建筑胶）&#xD;&#xA;4．C30混凝土台阶&#xD;&#xA;5．具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸，以台阶（包括最上层踏步边沿加300mm)水平投影面积计算" Dw="m2" Sl="3.86" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="0112" Mc="墙、柱面装饰工程" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="12" Qdbm="011201001001" Mc="墙面一般抹灰" Xmtz="1．底层厚度、砂浆配合比：素水泥浆一道（内掺建筑胶），8厚DP M15预拌砂浆打底分遍赶平&#xD;&#xA;2．面层厚度、砂浆配合比：5厚DP M20预拌砂浆抹平,中间压入一层耐碱玻纤网格布&#xD;&#xA;3．具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="207.96" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="13" Qdbm="011207001001" Mc="墙面装饰板" Xmtz="1.面层材料品种、规格、品牌、颜色：2.0mm厚白色拉丝肌理铝板(背衬10mm铝蜂窝芯)&#xD;&#xA;2.按高度安装配套水平不锈钢挂件及调整水平垂直度&#xD;&#xA;3.龙骨：40*40*4镀锌钢架、8#镀锌槽钢、镀锌钢板、不锈钢螺栓等龙骨与墙面锚固&#xD;&#xA;4.含铝板墙面与周边检修门、灯箱等收口做法&#xD;&#xA;5.具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按饰面外围尺寸，以展开面积计算" Dw="m2" Sl="286.90" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="14" Qdbm="WB011209010001" Mc="玻璃幕墙" Xmtz="1．玻璃品种、规格、颜色：8+1.52PVB+8钢化夹胶玻璃&#xD;&#xA;2．固定方式：不锈钢接驳器&#xD;&#xA;3．龙骨：镀锌方管钢龙骨&#xD;&#xA;4．工程量包含立面及顶面工程量&#xD;&#xA;5．具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示框外围尺寸，以投影面积计算" Dw="m2" Sl="106.60" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="15" Qdbm="WB011209010002" Mc="玻璃雨篷" Xmtz="1．玻璃品种、规格、颜色：8+1.52PVB+8钢化夹胶玻璃&#xD;&#xA;2．固定方式：不锈钢接驳器&#xD;&#xA;3．龙骨：镀锌方管钢龙骨&#xD;&#xA;4．具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示框外围尺寸，以投影面积计算" Dw="m2" Sl="2.76" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="0113" Mc="天棚工程" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="16" Qdbm="WB011302005001" Mc="吊顶天棚" Xmtz="1.2.0厚白色铝板&#xD;&#xA;2.纵向镀锌钢50X50X1.5U型镀锌钢(喷黑色)(吊点附吊挂)中距&lt;1200mm&#xD;&#xA;3.横向镀锌钢50X50X1.5U型镀锌钢(喷黑色)中距&lt;1200mm&#xD;&#xA;4.100x200x10mm热镀锌钢板(M12不锈钢膨胀螺栓固定)，50mm镀锌角钢&#xD;&#xA;5.含天花与卷帘收口做法&#xD;&#xA;6.具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸以展开面积计算" Dw="m2" Sl="64.78" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="17" Qdbm="WB011302007001" Mc="格栅吊顶" Xmtz="1．面层材料品种、规格：100*100*1.5厚铝方通@200mm，专用挂件安装(间距根据金属板尺寸)螺栓连接&#xD;&#xA;2．吊架材料种类、规格：φ10吊筋@≤1000mm，50*50*1.5U型镀锌龙骨&#xD;&#xA;3.   含检修孔制作&#xD;&#xA;4．具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m2" Sl="181.93" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="0114" Mc="油漆、涂料、裱糊工程" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="18" Qdbm="011406001001" Mc="墙面抹灰面油漆" Xmtz="1．无机涂料两道&#xD;&#xA;2.   刷封闭底漆1道&#xD;&#xA;3．满刮厚柔性耐水腻子找平三遍&#xD;&#xA;4．具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="689.60" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="19" Qdbm="011406001002" Mc="天棚抹灰面油漆" Xmtz="1．喷无机涂料两道&#xD;&#xA;2.   刷封闭底漆一道&#xD;&#xA;3．满刮2厚面层耐水腻子找平&#xD;&#xA;4．板底3厚底基防裂腻子分遍刮平&#xD;&#xA;5.   素水泥浆一道甩毛（内掺建筑胶）&#xD;&#xA;6．具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="164.55" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="20" Qdbm="011406001003" Mc="墙面喷黑处理" Xmtz="1．部位：格栅吊顶上方墙面&#xD;&#xA;2．黑色无机涂料两面&#xD;&#xA;3．具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="138.39" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="21" Qdbm="011406001004" Mc="天棚面喷黑处理" Xmtz="1．部位：格栅吊顶上方天棚面和设备管线处&#xD;&#xA;2．黑色无机涂料两面&#xD;&#xA;3．具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="246.71" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="0115" Mc="其他装饰工程" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="22" Qdbm="011503001001" Mc="金属扶手、栏杆、栏板 " Xmtz="1．部位：楼梯栏杆&#xD;&#xA;2．高度：斜段1000mm，平直段1050mm&#xD;&#xA;3．扶手材料种类、规格、品牌：φ50*3不锈钢管扶手两道&#xD;&#xA;4．栏杆材料种类、规格、品牌：φ30*3不锈钢管立柱&#xD;&#xA;5．固定配件种类：含预埋件、不锈钢法兰等栏杆配件&#xD;&#xA;6．具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示，以扶手中心线长度（包括弯头长度）计算" Dw="m" Sl="22.49" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="23" Qdbm="011503001002" Mc="金属扶手、栏杆、栏板 " Xmtz="1．部位：台阶栏杆&#xD;&#xA;2．高度：1100mm&#xD;&#xA;3．扶手材料种类、规格、品牌：φ40*3不锈钢管&#xD;&#xA;4．栏杆材料种类、规格、品牌：φ30*2不锈钢管立杆，φ50*3不锈钢管立柱&#xD;&#xA;5．固定配件种类：含预埋件、不锈钢法兰、螺栓等栏杆配件&#xD;&#xA;6．具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示，以扶手中心线长度（包括弯头长度）计算" Dw="m" Sl="4.86" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="24" Qdbm="011207001002" Mc="检修暗门" Xmtz="1.面层材料品种、规格、品牌、颜色：同周边墙面（另计）&#xD;&#xA;2.40*30*1.4铝方管（表面氟碳喷涂），60*60*4钢方管、工字钢等 &#xD;&#xA;3.含不锈钢开启执手、不锈钢铰链、等&#xD;&#xA;4.具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按饰面外围尺寸，以展开面积计算" Dw="m2" Sl="14.26" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="25" Qdbm="050201004001" Mc="盖板" Xmtz="1．部位：排水沟盖板&#xD;&#xA;2．材料种类：3厚发纹不锈钢多孔板盖板（304#）&#xD;&#xA;3．具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按图示尺寸以长度计算" Dw="m2" Sl="0.84" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="26" Qdbm="050201004002" Mc="盖板" Xmtz="1．部位：集水坑盖板&#xD;&#xA;2．材料种类：成品钢盖板，详24J306图集4-5&#xD;&#xA;3．具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按图示尺寸以长度计算" Dw="m2" Sl="0.98" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="27" Qdbm="010802001002" Mc="防淹板" Xmtz="1．名称：铝合金防淹板&#xD;&#xA;2.   高度：800mm，宽度40mm&#xD;&#xA;3.   含T型通常铝合金嵌条，橡胶条嵌缝&#xD;&#xA;4.   具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按设计图示洞口尺寸，以面积计算" Dw="m" Sl="3.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="0117." Mc="措施项目" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="28" Qdbm="011701006001" Mc="满堂脚手架" Xmtz="1.部位：装饰满堂脚手架&#xD;&#xA;2.搭设高度：详见图纸，综合考虑&#xD;&#xA;3.脚手架材质：满足合肥市相关文件规定，投标单位依据施工组织设计方案及相关规范综合考虑&#xD;&#xA;4.投标单位根据现有的图纸资料、招标文件和施工规范等资料，必须满足合肥市相关文件规定，综合报价&#xD;&#xA;5.具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求" Gcnr="" Jsgz="按实际搭设的水平投影面积计算" Dw="m2" Sl="305.48" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
  </Qdxm>
  <Csxm>
    <ZjCs>
      <ZjCsMx Xh="1" Xmbm="JC-01" Mc="夜间施工增加费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0.5" Je="0" Bz="" Cslb="1" />
      <ZjCsMx Xh="2" Xmbm="JC-02" Mc="二次搬运费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="1" Je="0" Bz="" Cslb="2" />
      <ZjCsMx Xh="3" Xmbm="JC-03" Mc="冬雨季施工增加费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0.8" Je="0" Bz="" Cslb="3" />
      <ZjCsMx Xh="4" Xmbm="JC-04" Mc="已完工程及设备保护费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0.1" Je="0" Bz="" Cslb="4" />
      <ZjCsMx Xh="5" Xmbm="JC-05" Mc="工程定位复测费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="1" Je="0" Bz="" Cslb="5" />
      <ZjCsMx Xh="6" Xmbm="JC-06" Mc="非夜间施工照明费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0" Je="0" Bz="" Cslb="6" />
      <ZjCsMx Xh="7" Xmbm="JC-07" Mc="临时保护设施费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0.2" Je="0" Bz="" Cslb="7" />
      <ZjCsMx Xh="8" Xmbm="JC-08" Mc="赶工措施费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0" Je="0" Bz="" Cslb="8" />
    </ZjCs>
  </Csxm>
  <Qtxm>
    <QtxmMx Xh="1" Mc="暂列金额" Dw="项" Je="0" Bz="" Xmlb="1" />
    <QtxmMx Xh="2" Mc="专业工程暂估价" Dw="项" Je="0" Bz="" Xmlb="2" />
    <QtxmMx Xh="3" Mc="计日工" Dw="" Je="0" Bz="" Xmlb="3" />
    <QtxmMx Xh="4" Mc="总承包服务费" Dw="" Je="0" Bz="" Xmlb="4" />
  </Qtxm>
  <Zlje />
  <Clzg />
  <Zygczg />
  <Jrg>
    <JrgBt Xh="一" Mc="人工" Je="0" Lb="1" />
    <JrgBt Xh="二" Mc="材料" Je="0" Lb="2" />
    <JrgBt Xh="三" Mc="施工机械" Je="0" Lb="3" />
  </Jrg>
  <Zcbfwf>
    <ZcbfwfMx Xh="1" Mc="发包人发包专业工程" Xmjz="0" Fwnr="" Fl="0" Je="0" />
    <ZcbfwfMx Xh="2" Mc="发包人供应材料" Xmjz="0" Fwnr="" Fl="0" Je="0" />
  </Zcbfwf>
  <Fbrgycl />
  <CbrgyclCef />
</Dwgcxx>
    <Dwgcxx Dwgcbh="0003" Dwgcmc="安装工程" Zylb="1" Jzmj="140" SoftName="国泰新点软件股份有限公司" SoftNum="30A18A095B562D6D2C1A60BC45D89196AA36B4B20D1E3F5B60A95DCE14113946CDB377BA186604044BEEF39BD7C006EF" DogNum="9733c801000702079e12000f002e001e" MachineKey="24418CF90623" Gcszd="市区">
  <Bkjzf>
    <BkjzfMx Xh="1.1" Bm="JF-01" Mc="    环境保护费" Qfjs="0" Fl="3.28" Je="0" Fyxlb="1.1" />
    <BkjzfMx Xh="1.2" Bm="JF-02" Mc="    文明施工费" Qfjs="0" Fl="5.12" Je="0" Fyxlb="1.2" />
    <BkjzfMx Xh="1.3" Bm="JF-03" Mc="    安全施工费" Qfjs="0" Fl="4.13" Je="0" Fyxlb="1.3" />
    <BkjzfMx Xh="1.4" Bm="JF-04" Mc="    临时设施费" Qfjs="0" Fl="8.1" Je="0" Fyxlb="1.4" />
    <BkjzfMx Xh="2.2" Bm="JF-05" Mc="  环境保护税" Qfjs="0" Fl="0" Je="0" Fyxlb="2.2" />
  </Bkjzf>
  <Sj>
    <SjMx Xh="1" Mc="税金" Qfjs="0" Jsjc="分部分项工程费+措施项目费+不可竞争费+其他项目费" Fl="9" Je="0" Fyxlb="1" />
  </Sj>
  <Qdxm>
    <QdBt Bm="1.1" Mc="消火栓系统" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="1" Qdbm="030901002001" Mc="消火栓钢管" Xmtz="1．名称：内外热镀锌钢管&#xD;&#xA;2．材质、规格：DN150&#xD;&#xA;3．连接形式：沟槽式连接&#xD;&#xA;4．含管道管件，开槽及恢复，与原管道接驳等工序&#xD;&#xA;5．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="47.25" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="2" Qdbm="030901002002" Mc="消火栓钢管" Xmtz="1．名称：内外热镀锌钢管&#xD;&#xA;2．材质、规格：DN65&#xD;&#xA;3．连接形式：沟槽式连接&#xD;&#xA;4．含管道管件，开槽及恢复，与原管道接驳等工序&#xD;&#xA;5．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="44.33" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="3" Qdbm="031002001001" Mc="管道支吊架制作与安装" Xmtz="1．名称：管道支吊架制作与安装&#xD;&#xA;2．材质：金属&#xD;&#xA;3．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="以千克计量，按设计图示质量计算" Dw="kg" Sl="104.98" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="4" Qdbm="031201003001" Mc="金属结构刷油" Xmtz="1．名称：管道支吊架刷油&#xD;&#xA;2．油漆品种：除锈清洁后,均刷防锈漆两道&#xD;&#xA;3．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="1．以平方米计量，按设计图示表面积尺寸以面积计算2．以千克计量，按金属结构的理论质量计算" Dw="kg" Sl="104.98" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="5" Qdbm="WB031003001001" Mc="沟槽阀门" Xmtz="1．名称：蝶阀&#xD;&#xA;2．材质：铸铁&#xD;&#xA;3．规格、压力等级：DN150&#xD;&#xA;4．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="6" Qdbm="030901010001" Mc="室内消火栓" Xmtz="1．名称：减压稳压型薄型单栓带消防软管卷盘组合式消防柜(不锈钢1800x700x180)&#xD;&#xA;2．型号、规格：内配DN65旋转消火栓1个,DN65,25m长衬胶水带一条,DN19mm水枪一支,30m长消防卷盘一套,自带4具灭火器&#xD;&#xA;3．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="7" Qdbm="030901013001" Mc="灭火器" Xmtz="1．名称：灭火器箱&#xD;&#xA;2．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="8" Qdbm="030901013002" Mc="灭火器" Xmtz="1．名称：灭火器&#xD;&#xA;2．规格、型号：MFABC-5&#xD;&#xA;3．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示数量计算" Dw="具" Sl="2.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="9" Qdbm="031201001001" Mc="管道刷油" Xmtz="1．名称：管道刷油&#xD;&#xA;2．油漆品种：刷规定颜色的调和漆两道&#xD;&#xA;3．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="1.以平方米计量，按设计图示表面积尺寸以面积计算2.以米计算，按设计图示尺寸以长度计算" Dw="m2" Sl="35.01" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="10" Qdbm="031208002001" Mc="管道绝热" Xmtz="1．名称：管道绝热&#xD;&#xA;2．绝热材料品种：离心玻璃棉管壳保温材料(50mm厚、憎水型)，外包不燃性玻璃布复合铝箔防潮层&#xD;&#xA;3．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按图示表面积加绝热层厚度及调整系数计算" Dw="m3" Sl="2.575" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="11" Qdbm="031208007001" Mc="防潮层、保护层" Xmtz="1．名称：保护层&#xD;&#xA;2．材料：铝合金薄板保护层(保护层厚度为0.6mm)&#xD;&#xA;3．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="1.以立方米计算，按图示表面积加绝热层厚度及调整系数计算2.以千克计量，按图示金属结构质量计算" Dw="m2" Sl="67.58" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="12" Qdbm="030905002001" Mc="水灭火系统控制装置调试" Xmtz="1．名称：消火栓系统调试&#xD;&#xA;2．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按控制装置的点数计算" Dw="项" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="1.2" Mc="压力排水系统" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="13" Qdbm="031001002001" Mc="钢管" Xmtz="1．名称：内外涂环氧树脂钢管&#xD;&#xA;2．规格、压力等级：DN100&#xD;&#xA;3．连接形式：卡箍连接&#xD;&#xA;4．含管道管件，开槽及恢复，与原管道接驳等工序&#xD;&#xA;5．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="84.09" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="14" Qdbm="031001002002" Mc="钢管" Xmtz="1．名称：内外涂环氧树脂钢管&#xD;&#xA;2．规格、压力等级：DN80&#xD;&#xA;3．连接形式：卡箍连接&#xD;&#xA;4．含管道管件，开槽及恢复，与原管道接驳等工序&#xD;&#xA;5．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="15.82" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="15" Qdbm="031001002003" Mc="钢管" Xmtz="1．名称：内外涂环氧树脂钢管&#xD;&#xA;2．规格、压力等级：DN65&#xD;&#xA;3．连接形式：卡箍连接&#xD;&#xA;4．含管道管件，开槽及恢复，与原管道接驳等工序&#xD;&#xA;5．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="5.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="16" Qdbm="031002001002" Mc="管道支吊架制作与安装" Xmtz="1．名称：管道支吊架制作与安装&#xD;&#xA;2．材质：金属&#xD;&#xA;3．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="以千克计量，按设计图示质量计算" Dw="kg" Sl="82.59" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="17" Qdbm="031201003002" Mc="金属结构刷油" Xmtz="1．名称：管道支吊架刷油&#xD;&#xA;2．油漆品种：除锈清洁后,均刷防锈漆两道&#xD;&#xA;3．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="1．以平方米计量，按设计图示表面积尺寸以面积计算2．以千克计量，按金属结构的理论质量计算" Dw="kg" Sl="82.59" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="18" Qdbm="WB031003001002" Mc="沟槽阀门" Xmtz="1．名称：绝缘接头&#xD;&#xA;2．规格、压力等级：DN125&#xD;&#xA;3．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="19" Qdbm="WB031003001003" Mc="沟槽阀门" Xmtz="1．名称：弹性座封闸阀&#xD;&#xA;2．规格、压力等级：DN80，PN10&#xD;&#xA;3．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="20" Qdbm="WB031003001004" Mc="沟槽阀门" Xmtz="1．名称：橡胶瓣膜止回阀&#xD;&#xA;2．规格、压力等级：DN80，PN10&#xD;&#xA;3．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="21" Qdbm="WB031003001005" Mc="沟槽阀门" Xmtz="1．名称：可曲挠橡胶接头&#xD;&#xA;2．规格、压力等级：DN80，PN10&#xD;&#xA;3．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="22" Qdbm="WB031003001006" Mc="沟槽阀门" Xmtz="1．名称：快速排水接头&#xD;&#xA;2．规格、压力等级：DN65&#xD;&#xA;3．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="23" Qdbm="031003011001" Mc="法兰" Xmtz="1．名称：法兰&#xD;&#xA;2．规格、压力等级：DN100&#xD;&#xA;3．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示数量计算" Dw="副" Sl="1.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="24" Qdbm="031003011002" Mc="法兰" Xmtz="1．名称：法兰&#xD;&#xA;2．规格、压力等级：DN80&#xD;&#xA;3．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示数量计算" Dw="副" Sl="9.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="25" Qdbm="031003011003" Mc="法兰" Xmtz="1．名称：法兰&#xD;&#xA;2．规格、压力等级：DN65&#xD;&#xA;3．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示数量计算" Dw="副" Sl="2.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="26" Qdbm="030601002001" Mc="压力仪表" Xmtz="1．名称：隔膜压力表&#xD;&#xA;2．配一个DN15的旋塞阀&#xD;&#xA;3．规格：YTP-100，0-0.6MPa&#xD;&#xA;4．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按图示数量计算" Dw="块" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="27" Qdbm="031004014001" Mc="给、排水附（配）件" Xmtz="1．名称：地漏&#xD;&#xA;2．型号、规格：DN100&#xD;&#xA;3．材质：不锈钢,水封不小于50mm&#xD;&#xA;4．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="28" Qdbm="030109001001" Mc="离心泵" Xmtz="1．名称：潜污泵&#xD;&#xA;2．规格：Q=36m3/h,H=0.20MPa,N=5.5kWTD/FSB-01,TD/FSB-02FSB-S1213-B1,FSB-S1213-B2&#xD;&#xA;3．含控制箱，防水电缆安装等工序&#xD;&#xA;4．潜污泵组包括潜污泵、控制柜、液位传感器(包括浮球式液位计、投入式液位计),控制柜至泵组、液位传感器的电力电缆、信号及控制电缆和其它辅助材料(不含预埋的配线管)起吊钢丝绳,潜水泵自动耦合装置等。控制柜内含双电源切换开关。&#xD;&#xA;5．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="29" Qdbm="031002003001" Mc="套管制作与安装" Xmtz="1．名称：柔性防水套管&#xD;&#xA;2．规格：DN125&#xD;&#xA;3．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="30" Qdbm="031208002002" Mc="管道绝热" Xmtz="1．名称：管道绝热&#xD;&#xA;2．绝热材料品种：离心玻璃棉管壳保温材料(50mm厚、憎水型)，外包不燃性玻璃布复合铝箔防潮层&#xD;&#xA;3．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按图示表面积加绝热层厚度及调整系数计算" Dw="m3" Sl="2.62" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="31" Qdbm="031208007002" Mc="防潮层、保护层" Xmtz="1．名称：保护层&#xD;&#xA;2．材料：铝合金薄板保护层(保护层厚度为0.6mm)&#xD;&#xA;3．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="1.以立方米计算，按图示表面积加绝热层厚度及调整系数计算2.以千克计量，按图示金属结构质量计算" Dw="m2" Sl="70.05" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="2.1" Mc="强电系统" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="32" Qdbm="030412001001" Mc="普通灯具" Xmtz="1．名称：LED壁灯&#xD;&#xA;2．规格：220V 1×18W LED&#xD;&#xA;3．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="7" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="33" Qdbm="030412004001" Mc="装饰灯" Xmtz="1．名称：LED嵌入式条形灯&#xD;&#xA;2．规格：宽150mm*高50mm 25W/米&#xD;&#xA;3．安装形式：吸顶安装&#xD;&#xA;4．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示数量计算" Dw="m" Sl="91.16" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="34" Qdbm="030412005001" Mc="荧光灯" Xmtz="1．名称：壁装式LED平板灯&#xD;&#xA;2．规格：220V 1×18W LED平板灯 1200x200mm&#xD;&#xA;3．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="35" Qdbm="030404034001" Mc="照明开关" Xmtz="1．名称：自熄式开关&#xD;&#xA;2．规格：250V 10A&#xD;&#xA;3．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="8" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="36" Qdbm="030411006001" Mc="接线盒" Xmtz="1．名称：接线盒&#xD;&#xA;2．材质：钢制&#xD;&#xA;3．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="52" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="37" Qdbm="030411001001" Mc="配管" Xmtz="1．名称：明敷配管&#xD;&#xA;2．规格：SC20&#xD;&#xA;3．含配管穿墙开孔及恢复等工序&#xD;&#xA;4．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="356.84" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="38" Qdbm="030411001002" Mc="配管" Xmtz="1．名称：明敷配管&#xD;&#xA;2．规格：SC25&#xD;&#xA;3．含配管穿墙开孔及恢复等工序&#xD;&#xA;4．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="130.50" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="39" Qdbm="030411001003" Mc="配管" Xmtz="1．名称：明敷配管&#xD;&#xA;2．规格：SC50&#xD;&#xA;3．含配管穿墙开孔及恢复，开槽及恢复等工序&#xD;&#xA;4．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="112.83" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="40" Qdbm="030408001001" Mc="电力电缆" Xmtz="1．名称：电力电缆&#xD;&#xA;2．规格：WDZB-YJY- 5X16&#xD;&#xA;3．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示尺寸以单相长度计算（含预留长度及附加长度）" Dw="m" Sl="487.01" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="41" Qdbm="030408006001" Mc="电力电缆头" Xmtz="1．名称：电力电缆头&#xD;&#xA;2．规格：16mm2&#xD;&#xA;3．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="42" Qdbm="030411004001" Mc="配线" Xmtz="1．名称：配线&#xD;&#xA;2．规格：WDZB-BYJ-2.5&#xD;&#xA;3．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示尺寸以单线长度计算（含预留长度）" Dw="m" Sl="2513.43" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="43" Qdbm="030411004002" Mc="配线" Xmtz="1．名称：配线&#xD;&#xA;2．规格：WDZBN-BYJ-2.5&#xD;&#xA;3．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示尺寸以单线长度计算（含预留长度）" Dw="m" Sl="657.55" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="44" Qdbm="030411004003" Mc="配线" Xmtz="1．名称：配线&#xD;&#xA;2．规格：WDZB1-RYJYSP-2*1.0&#xD;&#xA;3．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示尺寸以单线长度计算（含预留长度）" Dw="m" Sl="217.98" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="45" Qdbm="030414002001" Mc="送配电装置系统" Xmtz="1．名称：送配电装置系统&#xD;&#xA;2．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示系统计算" Dw="项" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="2.2" Mc="应急照明系统" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="46" Qdbm="WB030904013001" Mc="智能照明灯/指示灯" Xmtz="1．名称：安全出口标志灯&#xD;&#xA;2．规格：1W LED DC36V A型灯具&#xD;&#xA;3．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="47" Qdbm="WB030904013002" Mc="智能照明灯/指示灯" Xmtz="1．名称：安全疏散标志灯&#xD;&#xA;2．规格：1W LED DC36V A型灯具&#xD;&#xA;3．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="48" Qdbm="WB030904013003" Mc="智能照明灯/指示灯" Xmtz="1．名称：单向疏散指示标志灯&#xD;&#xA;2．规格：1W LED DC36V A型灯具&#xD;&#xA;3．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="28" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="49" Qdbm="WB030904013004" Mc="智能照明灯/指示灯" Xmtz="1．名称：地面电光型疏散指示标志灯&#xD;&#xA;2．规格：1W LED DC36V A型灯具 IP67 地面安装&#xD;&#xA;3．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="35" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="50" Qdbm="WB030904013005" Mc="智能照明灯/指示灯" Xmtz="1．名称：消防应急灯&#xD;&#xA;2．规格：5W LED DC36V A型灯具&#xD;&#xA;3．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="13" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="51" Qdbm="WB030904013006" Mc="智能照明灯/指示灯" Xmtz="1．名称：消防应急灯&#xD;&#xA;2．规格：10W LED DC36V A型灯具&#xD;&#xA;3．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="9" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="52" Qdbm="WB030904013007" Mc="智能照明灯/指示灯" Xmtz="1．名称：楼层指示灯&#xD;&#xA;2．规格：1W LED DC36V A型灯具&#xD;&#xA;3．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="53" Qdbm="WB030904013008" Mc="智能照明灯/指示灯" Xmtz="1．名称：双面单相疏散指示灯&#xD;&#xA;2．规格：1W LED DC36V A型灯具&#xD;&#xA;3．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="54" Qdbm="030411006002" Mc="接线盒" Xmtz="1．名称：接线盒&#xD;&#xA;2．材质：钢制&#xD;&#xA;3．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="92" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="55" Qdbm="030411001004" Mc="配管" Xmtz="1．名称：明敷配管&#xD;&#xA;2．规格：SC25&#xD;&#xA;3．含配管穿墙开孔及恢复等工序&#xD;&#xA;4．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="311.59" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="56" Qdbm="030408001002" Mc="电力电缆" Xmtz="1．名称：电力电缆&#xD;&#xA;2．规格：WDZBN-RYJYSP-2*2.5&#xD;&#xA;3．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示尺寸以单相长度计算（含预留长度及附加长度）" Dw="m" Sl="361.90" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="57" Qdbm="030408001003" Mc="电力电缆" Xmtz="1．名称：电力电缆&#xD;&#xA;2．规格：WDZBN-RYJYSP-2*4&#xD;&#xA;3．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示尺寸以单相长度计算（含预留长度及附加长度）" Dw="m" Sl="280.61" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="58" Qdbm="030408001004" Mc="电力电缆" Xmtz="1．名称：电力电缆&#xD;&#xA;2．规格：WDZAN-耐腐蚀橡胶绝缘电缆-2*2.5  &#xD;&#xA;3．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示尺寸以单相长度计算（含预留长度及附加长度）" Dw="m" Sl="315.23" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="59" Qdbm="030408006002" Mc="电力电缆头" Xmtz="1．名称：电力电缆头&#xD;&#xA;2．规格：≤10mm2&#xD;&#xA;3．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="2.3" Mc="消防电系统" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="60" Qdbm="030904006001" Mc="消防报警电话插孔（电话）" Xmtz="1．名称：手动火灾报警按钮（带电话插孔）&#xD;&#xA;2．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="61" Qdbm="030904003001" Mc="按钮" Xmtz="1．名称：消火栓火灾报警按钮&#xD;&#xA;2．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="62" Qdbm="030904001001" Mc="点型探测器" Xmtz="1．名称：点型感烟火灾探测器&#xD;&#xA;2．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="9" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="63" Qdbm="030904001002" Mc="点型探测器" Xmtz="1．名称：点型智能光电感烟探测器&#xD;&#xA;2．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="11" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="64" Qdbm="030904005001" Mc="声光报警器" Xmtz="1．名称：火灾声光警报器&#xD;&#xA;2．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="65" Qdbm="030411006003" Mc="接线盒" Xmtz="1．名称：接线盒&#xD;&#xA;2．材质：钢制&#xD;&#xA;3．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="31" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="66" Qdbm="030411001005" Mc="配管" Xmtz="1．名称：明敷配管&#xD;&#xA;2．规格：SC25&#xD;&#xA;3．含配管穿墙开孔及恢复等工序&#xD;&#xA;4．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="433.84" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="67" Qdbm="030411004004" Mc="配线" Xmtz="1．名称：配线&#xD;&#xA;2．规格：WDZB1N-RYJYSP-2*1.5mm2&#xD;&#xA;3．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示尺寸以单线长度计算（含预留长度）" Dw="m" Sl="245.96" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="68" Qdbm="030411004005" Mc="配线" Xmtz="1．名称：配线&#xD;&#xA;2．规格：WDZB1N-RYJYSP-2*2.5mm2&#xD;&#xA;3．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示尺寸以单线长度计算（含预留长度）" Dw="m" Sl="61.74" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="69" Qdbm="030408002001" Mc="控制电缆" Xmtz="1．名称：控制电缆&#xD;&#xA;2．规格：WDZB1N-KYJYP-2*1.5mm2&#xD;&#xA;3．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示尺寸以单相长度计算（含预留长度及附加长度）" Dw="m" Sl="464.44" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="70" Qdbm="030408007001" Mc="控制电缆头" Xmtz="1．名称：控制电缆头&#xD;&#xA;2．规格：2*1.5mm2&#xD;&#xA;3．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="71" Qdbm="030905001001" Mc="自动报警系统装置调试" Xmtz="1．名称：自动报警系统装置调试&#xD;&#xA;2．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按系统计算" Dw="项" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="72" Qdbm="030411004006" Mc="配线" Xmtz="1．名称：配线&#xD;&#xA;2．规格：WDZB1-RYJYP2*0.75&#xD;&#xA;3．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示尺寸以单线长度计算（含预留长度）" Dw="m" Sl="28.65" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="73" Qdbm="030411004007" Mc="配线" Xmtz="1．名称：配线&#xD;&#xA;2．规格：WDZB1-RYJYP6*0.75&#xD;&#xA;3．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示尺寸以单线长度计算（含预留长度）" Dw="m" Sl="57.30" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="74" Qdbm="030411004008" Mc="配线" Xmtz="1．名称：配线&#xD;&#xA;2．规格：WDZB1-RYJYP2*1.5&#xD;&#xA;3．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示尺寸以单线长度计算（含预留长度）" Dw="m" Sl="28.65" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="75" Qdbm="030411004009" Mc="配线" Xmtz="1．名称：配线&#xD;&#xA;2．规格：WDZB1-RYJYSP-2*1.0&#xD;&#xA;3．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示尺寸以单线长度计算（含预留长度）" Dw="m" Sl="102.07" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="76" Qdbm="030408001005" Mc="电力电缆" Xmtz="1．名称：电力电缆&#xD;&#xA;2．规格：WDZB1N-YJY -1*6.0&#xD;&#xA;3．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示尺寸以单相长度计算（含预留长度及附加长度）" Dw="m" Sl="50.85" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="77" Qdbm="030408001006" Mc="电力电缆" Xmtz="1．名称：电力电缆&#xD;&#xA;2．规格：WDZB1N-YJY 3*2.5&#xD;&#xA;3．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示尺寸以单相长度计算（含预留长度及附加长度）" Dw="m" Sl="304.94" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="78" Qdbm="030408006003" Mc="电力电缆头" Xmtz="1．名称：电力电缆头&#xD;&#xA;2．规格：≤10mm2&#xD;&#xA;3．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="6" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="79" Qdbm="030411001006" Mc="配管" Xmtz="1．名称：明敷配管&#xD;&#xA;2．规格：SC25&#xD;&#xA;3．含配管穿墙开孔及恢复等工序&#xD;&#xA;4．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="78.86" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="80" Qdbm="030411001007" Mc="配管" Xmtz="1．名称：明敷配管&#xD;&#xA;2．规格：SC32&#xD;&#xA;3．含配管穿墙开孔及恢复等工序&#xD;&#xA;4．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="203.72" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="2.4" Mc="防雷接地系统" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="81" Qdbm="030409002001" Mc="接地母线" Xmtz="1．名称：接地母线&#xD;&#xA;2．材质：40x4热镀锌扁钢&#xD;&#xA;3．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示尺寸以长度计算（含附加长度）" Dw="m" Sl="127.34" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="82" Qdbm="030414011001" Mc="接地装置" Xmtz="1．名称：防雷接地系统调试&#xD;&#xA;2．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="1．以系统计量，按设计图示系统计算2．以组计量，按设计图示数量计算。" Dw="项" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="3.1" Mc="防排烟系统" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="83" Qdbm="030702001001" Mc="碳钢通风管道" Xmtz="1．名称：矩形通风管道&#xD;&#xA;2．材质、厚度：镀锌钢管风管长边尺寸:450&lt;b≤1000,δ=0.75mm&#xD;&#xA;3．含管道穿墙设置套管，设置防火封堵等工序&#xD;&#xA;4．连接方式：角钢法兰连接&#xD;&#xA;5．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示内径尺寸以展开面积计算" Dw="m2" Sl="139.07" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="84" Qdbm="030703001001" Mc="碳钢阀门安装" Xmtz="1．名称：排烟防火阀&#xD;&#xA;2．规格：外形尺寸:1000x500,常开、280℃熔断关闭、手动复位、可输出信号&#xD;&#xA;3．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="分别按图示规格尺寸（直径或周长），以“个”为计量单位计算." Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="85" Qdbm="030703001002" Mc="碳钢阀门安装" Xmtz="1．名称：排烟防火阀&#xD;&#xA;2．规格：外形尺寸:800x500,常开、280℃熔断关闭、手动复位、可输出信号&#xD;&#xA;3．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="分别按图示规格尺寸（直径或周长），以“个”为计量单位计算." Dw="个" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="86" Qdbm="030703001003" Mc="碳钢阀门安装" Xmtz="1．名称：排烟阀&#xD;&#xA;2．规格：外形尺寸:1000x500,自带控制器以及线缆&#xD;&#xA;3．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="分别按图示规格尺寸（直径或周长），以“个”为计量单位计算." Dw="个" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="87" Qdbm="030703007001" Mc="碳钢风口、散流器、百叶窗" Xmtz="1．名称：单层百叶风口&#xD;&#xA;2．规格：外形尺寸:800*400,,钢制,配人字阀,带防护网(6X6)&#xD;&#xA;3．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="6" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="88" Qdbm="030703007002" Mc="碳钢风口、散流器、百叶窗" Xmtz="1．名称：单层百叶风口&#xD;&#xA;2．规格：外形尺寸:500*500,,铝合金,配人字阀,带防护网(6X6)&#xD;&#xA;3．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="6" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="89" Qdbm="031208003001" Mc="通风管道绝热" Xmtz="1．名称：岩棉保温&#xD;&#xA;2．绝热材料品种：密度120kg/m3，导热系数≤0.044W/(m·K),耐水阻燃贴面FFR(外层)&#xD;&#xA;3．绝热厚度：耐火极限1h厚度45mm，耐火极限3h厚度50mm&#xD;&#xA;4．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="1．以立方米计算，按图示表面积加绝热层厚度及调整系数计算2．以立方米计量，按图示表面积及调整系数计算" Dw="m3" Sl="7.69" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="90" Qdbm="031208007003" Mc="防潮层、保护层" Xmtz="1．名称：防火板&#xD;&#xA;2．厚度：耐火极限不低于3h,厚度12mm&#xD;&#xA;3．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="1.以立方米计算，按图示表面积加绝热层厚度及调整系数计算2.以千克计量，按图示金属结构质量计算" Dw="m2" Sl="158.73" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="3.2" Mc="空调系统" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="91" Qdbm="030701003001" Mc="空调器" Xmtz="1．名称：室内机&#xD;&#xA;2．规格：CL=10kW,N=0.2kW,四面出风嵌入式,配冷凝水提升泵,带回风过滤网&#xD;&#xA;3．含多联机集控器，有线控制器，网关等&#xD;&#xA;4．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="92" Qdbm="031001004001" Mc="铜管" Xmtz="1．名称：冷媒管&#xD;&#xA;2．规格、压力等级：紫铜管φ9.5&#xD;&#xA;3．连接形式：承插焊接&#xD;&#xA;4．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="23.55" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="93" Qdbm="031001004002" Mc="铜管" Xmtz="1．名称：冷媒管&#xD;&#xA;2．规格、压力等级：紫铜管φ12.7&#xD;&#xA;3．连接形式：承插焊接&#xD;&#xA;4．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="10.02" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="94" Qdbm="031001004003" Mc="铜管" Xmtz="1．名称：冷媒管&#xD;&#xA;2．规格、压力等级：紫铜管φ15.9&#xD;&#xA;3．连接形式：承插焊接&#xD;&#xA;4．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="17.89" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="95" Qdbm="031001004004" Mc="铜管" Xmtz="1．名称：冷媒管&#xD;&#xA;2．规格、压力等级：紫铜管φ19.1&#xD;&#xA;3．连接形式：承插焊接&#xD;&#xA;4．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="13.46" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="96" Qdbm="031001004005" Mc="铜管" Xmtz="1．名称：冷媒管&#xD;&#xA;2．规格、压力等级：紫铜管φ22.2&#xD;&#xA;3．连接形式：承插焊接&#xD;&#xA;4．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="10.09" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="97" Qdbm="031001004006" Mc="铜管" Xmtz="1．名称：冷媒管&#xD;&#xA;2．规格、压力等级：紫铜管φ28.6&#xD;&#xA;3．连接形式：承插焊接&#xD;&#xA;4．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="27.91" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="98" Qdbm="031001001001" Mc="镀锌钢管" Xmtz="1．名称：镀锌钢管&#xD;&#xA;2．规格、压力等级：DN20&#xD;&#xA;3．连接形式：螺纹连接&#xD;&#xA;4．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="16.68" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="99" Qdbm="031002001003" Mc="管道支吊架制作与安装" Xmtz="1．名称：管道支吊架制作与安装&#xD;&#xA;2．材质：金属&#xD;&#xA;3．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="以千克计量，按设计图示质量计算" Dw="kg" Sl="132.97" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="100" Qdbm="031201003003" Mc="金属结构刷油" Xmtz="1．名称：管道支吊架刷油&#xD;&#xA;2．油漆品种：除锈清洁后,均刷防锈漆两道&#xD;&#xA;3．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="1．以平方米计量，按设计图示表面积尺寸以面积计算2．以千克计量，按金属结构的理论质量计算" Dw="kg" Sl="132.97" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="101" Qdbm="030804010001" Mc="低压铜及铜合金管件" Xmtz="1．名称：铜管分歧器&#xD;&#xA;2．规格：外径(mm以内) 30&#xD;&#xA;3．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="102" Qdbm="030411003001" Mc="桥架" Xmtz="1．名称：冷媒桥架&#xD;&#xA;2．规格：200X100，镀锌钢板厚度2.0mm&#xD;&#xA;3．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="48.62" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="103" Qdbm="030413001001" Mc="铁构件" Xmtz="1．名称：桥架支吊架&#xD;&#xA;2．材质：金属&#xD;&#xA;3．含除锈刷油等工序&#xD;&#xA;4．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示尺寸以质量计算" Dw="t" Sl="0.058" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="104" Qdbm="031208002003" Mc="管道绝热" Xmtz="1．名称：管道保温&#xD;&#xA;2．绝热材料品种：复合型橡塑保温&#xD;&#xA;3．绝热厚度：冷媒管20mm，冷凝管15mm&#xD;&#xA;4．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按图示表面积加绝热层厚度及调整系数计算" Dw="m3" Sl="0.263" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="105" Qdbm="WB031002008001" Mc="抗震支架安装" Xmtz="1．名称：抗震支架安装&#xD;&#xA;2．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="按设计图示数量计算" Dw="项" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="106" Qdbm="031301012001" Mc="工程系统检测、检验" Xmtz="1．名称：工程系统检测、检验&#xD;&#xA;2．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="" Dw="项" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="107" Qdbm="031301017001" Mc="脚手架搭拆" Xmtz="1．名称：脚手架搭拆&#xD;&#xA;2．其他未尽事宜详见设计图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求等" Gcnr="" Jsgz="" Dw="项" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
  </Qdxm>
  <Csxm>
    <ZjCs>
      <ZjCsMx Xh="1" Xmbm="JC-01" Mc="夜间施工增加费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0.5" Je="0" Bz="" Cslb="1" />
      <ZjCsMx Xh="2" Xmbm="JC-02" Mc="二次搬运费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="1" Je="0" Bz="" Cslb="2" />
      <ZjCsMx Xh="3" Xmbm="JC-03" Mc="冬雨季施工增加费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0.8" Je="0" Bz="" Cslb="3" />
      <ZjCsMx Xh="4" Xmbm="JC-04" Mc="已完工程及设备保护费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0.1" Je="0" Bz="" Cslb="4" />
      <ZjCsMx Xh="5" Xmbm="JC-05" Mc="工程定位复测费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="1" Je="0" Bz="" Cslb="5" />
      <ZjCsMx Xh="6" Xmbm="JC-06" Mc="非夜间施工照明费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0" Je="0" Bz="" Cslb="6" />
      <ZjCsMx Xh="7" Xmbm="JC-07" Mc="临时保护设施费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0.2" Je="0" Bz="" Cslb="7" />
      <ZjCsMx Xh="8" Xmbm="JC-08" Mc="赶工措施费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0" Je="0" Bz="" Cslb="8" />
    </ZjCs>
  </Csxm>
  <Qtxm>
    <QtxmMx Xh="1" Mc="暂列金额" Dw="项" Je="0" Bz="" Xmlb="1" />
    <QtxmMx Xh="2" Mc="专业工程暂估价" Dw="项" Je="0" Bz="" Xmlb="2" />
    <QtxmMx Xh="3" Mc="计日工" Dw="" Je="0" Bz="" Xmlb="3" />
    <QtxmMx Xh="4" Mc="总承包服务费" Dw="" Je="0" Bz="" Xmlb="4" />
  </Qtxm>
  <Zlje />
  <Clzg />
  <Zygczg />
  <Jrg>
    <JrgBt Xh="一" Mc="人工" Je="0" Lb="1" />
    <JrgBt Xh="二" Mc="材料" Je="0" Lb="2" />
    <JrgBt Xh="三" Mc="施工机械" Je="0" Lb="3" />
  </Jrg>
  <Zcbfwf>
    <ZcbfwfMx Xh="1" Mc="发包人发包专业工程" Xmjz="0" Fwnr="" Fl="0" Je="0" />
    <ZcbfwfMx Xh="2" Mc="发包人供应材料" Xmjz="0" Fwnr="" Fl="0" Je="0" />
  </Zcbfwf>
  <Fbrgycl />
  <CbrgyclCef />
</Dwgcxx>
  </Dxgcxx>
</JingJiBiao>